EF-EL Airbag codes

Hi mate,

I have the same problem. When the light is flashing that is your fault codes. You need to count them. It will flash, then there will be a slight pause then it will flash again, then it will stay on all the time. eg 5 flashes, pause, 3 flashes, constant illumination.
That is the code mine flashes up and I'll be checking it out in the next few days.

Here are the codes:

FORD FALCON EF 1994-96 SRS Safety Restraint System (Airbag)
FORD FALCON EL 1996-98 SRS Safety Restraint System (Airbag)
Also suits Fairmont, XR6, XR8, Fairlane NF & NL and LTD DF & DL Models
Fault Codes
Vehicles built from November 1994-ON:
Will flash the Fault Codes as they are detected by the ECM via the SRS Checklamp
Fault Codes must be retrieved manually.
Start the Engine
The Airbag (SRS) Checklight will stay on for 6 to 8 Seconds and then extinguish.
(This indicates the System is operational with no Faults.)
Faults in the System will cause the Checklight to:
1. Not illuminate
2. Constantly illuminate or
3. Flash the Fault Codes
The Checklight will not register a Fault for 30 to 45 Seconds after the Ignition is switched ON.
Fault Codes are displayed as flashes of the Airbag Checklight.
Example:
Fault Code 24 is represented by:
2 Flashes
(2 Second interval)
4 Flashes
(5 Second interval)
The Code is then repeated.
The Fault Codes are organised into two groups
1. The Hard Codes 
These represent the Fault Codes
(Codes 12 to 45)

2. The Repaired Codes (Or Intermittent Codes)
These have 40 added to the Hard Codes (12 + 40 = 52)
(Codes 52 to 85).
Example:
Hard Fault Code 12 (Low Battery Voltage) becomes;

Repaired Fault Code 52 (When Repaired
Fault Code Erasure
The Hard Codes are NOT Erasable.
Only the Repaired or Intermittent Codes are erasable.
Faults pertaining to the Hard Fault Codes must first be repaired.
This Converts the Hard Fault Code to a "Repaired Fault Code" and is NOW Erasable.
Example:
If Code 12 (low battery voltage) was displayed (Problem - Faulty Battery)
It is NON-erasable.
The Battery is subsequently changed.
The ECM now sees that the Battery Volts are OK.
It adds 40 to the Hard Fault Code 12 and displays (12 + 40 = 52)
Repaired Fault Code 52 (Repaired or Intermittent Code).
Because the Fault has been repaired, the Fault Code can be erased from the memory.
This principle applies to all Airbag components.
To Erase Codes:
1. Carry out Fault Code Extraction
2. When the Codes are flashing;
Connect a Jumper Wire between the Airbag Memory Clear Pin and a Suitable Ground.
3. Wait for 5 "Beeps" to sound.
4. Disconnect Jumper Wire.
5. Switch Ignition OFF.
6. Carry out Fault Code Extraction for further Codes.
7. Repeat this Procedure to erase subsequent Codes
If the Jumper Wire is NOT removed before the Ignition is switched OFF;
Fault Codes will NOT be cleared.
Fault Code Extraction
Switch Ignition ON
Wait until the Checklight extinguishes. (6 to 8 Seconds)
Wait for 30 to 45 Seconds. 
One Fault Code will be displayed at a time. (Highest Priority First).
To Retrieve Successive Fault Codes:
1 The Fault indicated by the First Fault Code must be repaired.
2. The Fault Code must be erased.
3. Carry out Fault Code Extraction again.
4. The Next Highest Priority Fault Code will then be displayed. 
Fault Code Table (Hard Faults)
The Fault Codes are listed in order of Highest Priority.
Code # Circuit and Status
No Lamp Lamp Circuit
Continuous
Lamp Fault Code Timed Out
ECM Disconnected or Inoperative
NO Power to ECM

12 Low Battery Volts

13 Airbag Circuit
Shorted to Ground

14 Primary Impact Sensor
Shorted to Ground

21 ECM
Not Mounted to Vehicle Body

22 Safing Sensor
Shorted to Power

23 Memory Clear Circuit
Improperly Grounded

24 System Disarm Failure OR ECM Fault


32 Airbag Circuit Open OR High Resistance

33 Resistor High Resistance or Open Circuit
The Resistor is located on the Wiring Loom near the ECM

34 Airbag Circuit Shorted OR Low Resistance

35 Resistor Low Resistance or Shorted
The Resistor is located on the Wiring Loom near the ECM

41 Impact Sensor # 1 Feed
Return Open Circuit

42 Impact Sensor # 2 Feed
Return Open Circuit

44 Impact Sensor # 1
Not Mounted to Vehicle Correctly


45 Impact Sensor # 2
Not Mounted to Vehicle Correctl

Fault Code Table (Repaired Or Intermittent Codes)

This list is the same as the Hard Code List.

The only difference is that 40 has been added to each Component.

This indicates that the ECM is saying that the component has been;

1. Repaired OR

2. Has returned to its Original Preset (intermittent) State.

The Fault Codes are listed in order of Highest Priority

Code # Circuit and Status
52 Repaired or Intermittent Low Battery Voltage

53 Repaired or Intermittent Airbag Circuit Shorted to Ground

54 Repaired or Intermittent Primary Impact Sensor Shorted to Ground

61 Repaired or Intermittent ECM Not Mounted to Vehicle Body

62 Repaired or Intermittent Safing Sensor Circuit Shorted to Power

63 Repaired or Intermittent Memory Clear Circuit Improperly Grounded

64 Repaired or Intermittent System Disarm Failure OR ECM Fault


72 Repaired or Intermittent Airbag Circuit Open OR High Resistance

73 Repaired or Intermittent Resistor

74 Repaired or Intermittent Airbag Circuit Shorted OR Low Resistance

75 Repaired or Intermittent Resistor

81 Repaired or Intermittent Impact Sensor # 1 Feed
Return Open Circuit

82 Repaired or Intermittent Impact Sensor # 2 Feed 
Return Open Circuit

84 Repaired or Intermittent Impact Sensor # 1 
Not Mounted to Vehicle Correctly


85 Repaired or Intermittent Impact Sensor # 2 
Not Mounted to Vehicle Correctly

Continual 
Flashing Both Impact Sensors Disconnected 

"Beeps" Check Light Inoperative AND some Faults present 

FORD FALCON EF 1994-96 SRS Safety Restraint System (Airbag)

FORD FALCON EL 1996-98 SRS Safety Restraint System (Airbag)
Also suits Fairmont, XR6, XR8, Fairlane NF & NL and LTD DF & DL Models 

1. Mounted on the Radiator Support Panel (Approximately the Centre).
2. Mounted on the Brake Pedal Mounting Bracket directly above the Drivers Footrest.
(This is in Front of the Heater Duct)

The Impact Sensors do NOT need to be replaced in the event of Airbag Deployment.
They Automatically Reset themselves.

The Impact Sensors are Hard Wired to the Airbag.

The ECM also contains a Third Impact Sensor (Safing Sensor).
It also contains an Audible Alarm in case of SRS Checklamp Failure.
The Audible Alarm will sound;
5 sets of 5 Beeps every 40 Minutes. 

The Airbag will Deploy in a Front End (or Near Front End) Collision of;
Approximately the Impact Deceleration Force of 25 kph into a Brick Wall if:

1. Either (or Both) of the Impact Sensors are activated Plus
2. The Safing Sensor is activated Simultaneously.

Erase Pin
Turn on the ignition and wait for the Airbag light to start flashing, then earth the "airbag memory clear" pin of the diagnostic connector (4th pin from top left). When the code has cleared you will hear 3 beeps from the airbag monitor (hidden under dash, above fuse panel). Turn off the key (Noels Note-First on I did wouldn’t clear if earth removed while key still on?) Remove the earth wire and make sure the Airbag light stays out.

